Three-way thermostatic valve

1) Case material - stainless steel SS 316;

2) Diameter DN80;

3) Flange according to ASME B16.5, 150#RF;

4) Controlled temperature is 71.1°C (160°F), opening temperature is 68.3°C (155°F), full opening temperature is 78.3°C (173°F);

5) With additional manual control function.

6) Working pressure - 8.5 kg/cm2,

7) This equipment is intended for use in temperatures between -60°C and +60°C.

